**Flood forecasting using transboundary data with the fuzzy inference system: The Maritza (Meriç) River**

A. Aydın1, I. Yücedağ2 and R. Eker1,\*

[1] Düzce University, Faculty of Forestry, 81620 Düzce, Turkey

[2] Düzce University, Faculty of Technology, 81620 Düzce, Turkey

[\*] Corresponding author: Remzi Eker ([remzieker@duzce.edu.tr](mailto:remzieker@duzce.edu.tr))

Abstract

~~The rising floodwaters of the Maritza River, originating in the Balkans, affect those living in adjacent areas. The lower regions of the Maritza River are especially vulnerable to floods. The city of Edirne and the surrounding region in Turkey located downstream of the Maritza River are frequently affected by flooding. The section of the river inside the Turkish border is short; therefore, there is not adequate warning time for Turkey to alert the population against flash floods. For this reason, it is essential that Turkey acquire current flow information from Bulgarian sites for use in current flow prediction for Turkey’s section of the river.~~ ~~To this aim~~ In the present study, in order to predict the flood hydrograph of the Kirişhane station (Turkey) from the transboundary data of Plovdiv and Svilengrad stations (Bulgaria), four different models (M1‒M4) were developed by using the fuzzy inference system (FIS) for different number of membership functions (MFs) (i.e. 13, 25, and 49 MFs). In addition, multiple linear regression (MLR) was selected as simpler data driven forecasting method to show how FIS improves the other simpler forecasting models. Flow data from the Plovdiv, Svilengrad and Kirişhane stations were gauged at two hour-intervals covering the flood period from 9 February 2010 00:00:00 to 21 February 2010 22:00:00. In addition, flow data at two hour-intervals covering the flood period from 6 February 2012 14:00:00 to 13 February 2012 10:00:00 were obtained to test developed FIS and MLR models. In the first model, estimation was made using the current flows of the Plovdiv and Svilengrad stations. In the second model, estimation was made based on a two hour ahead prediction of the Svilengrad station and a four hour ahead prediction of the Plovdiv station. In the third model, calculations were based on predictions of four hours ahead of the Svilengrad station and eight hours ahead of the Plovdiv station. In the last model, estimation was based on predictions of six hours ahead of the Svilengrad station and twelve hours ahead of the Plovdiv station. ~~The prediction ability of the FIS was evaluated by using the determination coefficient (R2), the Nach-Sutcliffe sufficiency score (NSSS), the normalized root mean square error (NRMSE), and the correlation coefficient (CORR).~~ The performance of the developed FIS models and MLR was evaluated by using the mean absolute error (MAE), the Nach-Sutcliffe model efficiency coefficient (NSMEC), and the normalized root mean square error (NRMSE). According to the performance criteria of the models, FIS model with 49 number of MFs provided highest accuracy. When FIS models with 25 MFs and 49 MFs are compared with respect to performance criteria for 2010 data (training data), NSMEC values are close to each other, but MAE values of FIS models with 49 MFs were obtained less than FIS model with 25 MFs. Even though NSMEC values were obtained close to each other for FIS models with 25 MFs and 49 MFs, NSMEC values of FIS model with 25 MFs were obtained less than 0.90 for 2012 data (validation data). With respect to MLR, all models failed to predict 2012 data, even NSMEC values of MLR model were obtained higher than 0.85 for training data. Even the accuracy of FIS models decrease based on decrease in the number of MFs, all FIS models provided better prediction of 2012 data than MLR.

**Keywords:** FIS, flood hydrograph, streamflow forecasting, transboundary data, Maritza River

# 1. Introduction

In recent years, soft computing techniques have been increasingly used for forecasting studies in hydrology (Mukerji et al., 2009). Within flow regulation and water resources management studies, streamflow or flood forecasting have become a very demanding task which seeks to mitigate the effects of floods on human and dam safety as well as on ecosystem sustainability (Campolo et al., 1999; Lekkas et al., 2005). However, the process of forecasting streamflow or flood is a very complex hydrological process owing to the tremendous spatial and temporal variability in the characteristics of terrain and rainfall patterns in conjunction with other variables associated with modeling (Tokar and Markus, 2000; Nayak et al., 2005). Reliable water level forecasts enable the use of early warning systems to alert the population as well as real time control of hydraulic structures in order to mitigate the adverse effects when floods occur (Alvisi et al., 2006). Recording and analyzing the streamflow are indispensable procedures because they can generate significant indications of both past and future flow characteristics (Küçük and Ağıralioğlu, 2006). Furthermore, flood management studies require knowledge of the magnitude and frequency of high flows (Amisigo et al., 2008). Accurate and timely prediction of high and low flow events can provide the information required to make strategic decisions at any watershed location (Besaw et al., 2010). Hence, the forecasting of stream flows in real time has received noticeable attention from hydrologists and resource engineers for many decades (Chang and Chen, 2001).

To date, a wide variety of models for streamflow or flood forecasting have been developed and applied, ranging from completely black box models to very detailed conceptual models (Nayak et al., 2005). The methods used for forecasting gauged and/or ungauged streamflow are categorized as conceptual, metric, physics-based and data-driven (Besaw et al., 2010). Data-driven methods have been extensively adopted for forecasting streamflow or flood. Of the data-driven methods, multiple linear regression (MLR), auto-regressive moving average (ARMA), and artificial neural networks (ANNs) are commonly used models (McKerchar and Delleur, 1974; Chaloulakou et al., 1999; García-Bartual, 2002; Cığızoğlu, 2003; Yurekli et al., 2005; Fırat, 2008; Wang et al., 2008; Kar et al., 2010; Aydın and Eker, 2012; Rezaeianzadeh et al., 2014) because they require much less development time and are capable of more accurate prediction of streamflow (Govindaraju, 2000). In addition, fuzzy logic has been used in hydrological modeling for various applications (Altunkaynak et al., 2005; Nayak et al., 2005; Chen et al., 2006; Fırat and Güngör, 2007; Özger, 2009; Şen and Altunkaynak, 2009; Turan and Yurdusev, 2009). Fuzzy models enable nonlinear solutions in practice when the required number of fuzzy sets and rules is provided (Özger, 2009).

~~Floodwaters rising from the Maritza River, which is the biggest river on the Balkan Peninsula, affect Turkey, Greece, and Bulgaria. In particular, the lower regions of the Maritza River are vulnerable to floods because the physical and hydrological characteristics of the river create a high flooding potential. In Turkey, the city of Edirne and the surrounding region are prone to flooding. The flood of June 1911 was one of the biggest, with a maximum discharge of approximately 1500 m3/s (Tuncok, 2015). Some of the more recent floods documented include the ones in 1957 with 1200 m3/s and in 1976 with 783 m3/s in addition to those in 2005, 2006, and 2007 (Tuncok, 2015). Moreover, the flood occurring on 16 February 2010 is considered to be the second biggest flood in the last 26 years. During this flood, a maximum discharge of 1713 m3/s was measured in the city of Edirne, while 2800 m3/s was measured in Ipsala (Batur and Maktav, 2012).~~ ~~Turkey is unable to provide adequate warning time to alert the population against floods because the section of the river inside the country is short (Sezen et al., 2007). Thus, getting current flow information from Bulgarian sites and using it in the current prediction for Turkey’s section of the River is essential. The main aim of the present study was to develop a fuzzy model from flow data originating from three stations (Plovdiv and Svilengrad in Bulgaria and Kirişhane in Turkey) located on the Maritza River, and to show the capability of the developed models to use the transboundary data in the prediction of current streamflow.~~ In the literature, streamflow prediction studies are common, but flood forecasting studies are limited (e.g. Campolo et al., 1999; Mukerji et al., 2009; Kar et al., 2010; Rezaeianzadeh et al., 2014). That’s why, the main aim of the present study was to develop a fuzzy inference system from flow data available only for flood periods (which covers very short period several days) originating from three stations (Plovdiv and Svilengrad in Bulgaria and Kirişhane in Turkey) located on the Maritza River, and to show the capability of the developed models to use the transboundary data in the prediction of flood hydrographs.

# 2. Material and method

**~~2.1 Fuzzy logic~~**

~~Fuzzy logic, which was suggested by Zadeh in 1965, is a generalization of classical logic. The diﬀerence between fuzzy logic and crisp (i.e., classical) logic is established by introducing a membership function. A universal set X determined to be either members or non-members of a crisp set can be defined by a discrimination function and for a given crisp set A. This function, which can be indicated by, assigns the value to every as follows (Hong and Lee, 1996):~~

~~(1)~~

~~The membership function in fuzzy logic is a generalized form of the discriminant function; values assigned to elements in fuzzy sets fall within a specified range and are referred to as the membership grades of these elements. Membership function can be indicated by~~

~~(2)~~

~~where X refers to the universal set defined in a specific problem, and [0, l] denotes the interval of real numbers from 0 to 1, inclusively.~~

~~Although a great number of membership functions were developed in fuzzy logic, the most commonly used are the triangular, sigmoidal, trapezoidal, and Gaussian membership functions (Baykal and Beyan, 2004). The most extensively used primitives for fuzzy union and fuzzy intersection are max and min operators. Assuming that A and B are two fuzzy sets with membership functions of and, the fuzzy union and fuzzy intersection are as follows:~~

~~(3)~~

~~Fuzzy logic provides a very valuable ﬂexibility for reasoning which makes it possible to take into account inaccuracies and uncertainties. Additionally, fuzzy logic provides for the processing of linguistic knowledge and its corresponding numerical data through membership functions (Zadeh, 1973). Fuzzy models are capable of incorporating knowledge from human experts naturally and conveniently, while traditional models fail to do so (Yen and Langari, 1999). Moreover, fuzzy models have the ability to handle the nonlinearity and interpretability features of the models (Yen and Langari, 1999). Fuzzy models can be created from knowledge of experts by translating linguistic information into fuzzy rules (Yanar, 2010), albeit there is no standard method available for transforming this knowledge (Jang, 1993).~~

~~A basic fuzzy logic statement is made in a rule-based system and can appear in the form of IF‒THEN statements. A fuzzy inference system (FIS) can have both fuzzy sets and crisp values, but the outputs are always fuzzy sets. Hence, defuzzification is performed to convert fuzzy sets of outputs to crisp values. The general structure of an FIS is depicted in Fig. 1.~~

***2.1. Study area and dataset***

The Maritza River, which is 490 km long, originates at 2400 m a.s.l in the Rila Mountains (Bulgaria) and flows southeast for 320 km (Fig. 1). The catchment of the Maritza River has an area of 52600 km2, 28% of which is located in Turkey. After flowing along a short portion of the Greek‒Bulgarian border, the river arrives in Turkey, where it flows for 13 km, after which it forms the border between Turkey and Greece until it disembogues into the Aegean Sea (Yıldız et al., 2014). There are two main tributaries (Arda and Tundja rivers) can be effect the flow located before Kirişhane gauging station. The length of Tundja is approximately 390 km and the length of Arda is around 240 km. While Tundja has around 50 tributaries, Arda has around 25 tributaries (Tuncok et al., 2014).

Floodwaters rising from the Maritza River, which is the biggest river on the Balkan Peninsula, affect Turkey, Greece, and Bulgaria. In particular, the lower regions of the Maritza River are vulnerable to floods because the physical and hydrological characteristics of the river create a high flooding potential. In Turkey, the city of Edirne and the surrounding region are prone to flooding. The Maritza basin is under the influence of both the continental and the Mediterranean climates. The high flow period for the regions under the continental climatic influence can be observed in the northern part of Maritza basin and comes in late spring. On the other hand, the Mediterranean climatic influence is more visible to the south, affecting the lower parts of the Maritza and causing high flow conditions during winter. Flooding of the Maritza River typically occurs in the autumn, winter, and spring seasons and is caused mainly by heavy rainfalls and snowmelts (Tuncok, 2015).

The flood of June 1911 was one of the biggest, with a maximum discharge of approximately 1500 m3/s. Some of the more recent floods documented include the ones in 1957 with 1200 m3/s and in 1976 with 783 m3/s in addition to those in 2005, 2006, and 2007 (Tuncok, 2015). Moreover, the flood occurring on 16 February 2010 is considered to be the second biggest flood in the last 26 years. During this flood, a maximum discharge of 1713 m3/s was measured in the city of Edirne, while 2800 m3/s was measured in Ipsala (Batur and Maktav, 2012). Turkey is unable to provide adequate warning time to alert the population against floods because the section of the river inside the country is short (Sezen et al., 2007). Thus, getting current flow information from Bulgarian sites and using it in the current prediction for Turkey’s section of the River is essential.

Fig. 1 about here

In the present study, flow data from the Plovdiv and Svilengrad stations (Bulgaria), and the Kirişhane station (Turkey), all located on the Maritza River, were gauged at two hour-intervals covering the flood period from 9 February 2010 00:00:00 to 21 February 2010 22:00:00. In addition, flow data at two hour-intervals covering the flood period from 6 February 2012 14:00:00 to 13 February 2012 10:00:00 were obtained to test developed models. Streamflow is gauged in normal at eight hours-intervals along one year, however, flow data is gauged at two hour-intervals only during flood period. That’s why, flow data used in the present study is limited with several days. In addition, two hour-intervals of 2012 flow data is available for shorter period than 2010 flow data and available data period belongs to recession stage of flood as seen in the hydrograph (Fig. 2).

Fig. 2 about here

***2.1. Fuzzy Inference System***

Fuzzy Inference System (FIS), known in the literature as fuzzy rule based system, fuzzy expert system, or a fuzzy system, is the process of mapping from a given input set using fuzzy logic which was suggested by Zadeh in 1965 (Elsayed, 2009). Linguistic terms in a rule-based system are used.to provide an inference structure for modeling sophisticated and complex structures (Jamshidi et al., 2013). There are two types of widely used fuzzy inference systems, Takagi–Sugeno FIS and Mamdani FIS (Jang et al. 1997). The definition of the consequent parameters is the basic difference between these fuzzy inference systems (Takagi and Sugeno, 1985). In Takagi-Sugeno FIS, consequent parameters can be either a linear equation or a constant, whereas in Mamdani FIS, rule base is constructed from input-output pairs, which can have both fuzzy sets and crisp values, but the outputs are always fuzzy sets. In this study, Mamdani type inference were adopted. The general structure of FIS is depicted in Fig. 3. As shown in Fig. 3, FIS includes four main parts (1) fuzzification, (2) rule base, (3) decision making unit, and (4) defuzzification.

The fuzzification is the process of transforming crisp values into grades of membership for linguistic terms of fuzzy sets transferring crisp values into fuzzy If-Then rules. Transforming crisp values into fuzzy in the present study was made by the definition of flow data as SN (Small N),…, S1 (Small 1), CE (Center), B1 (Big 1),…, BN (Big N) adopted for Triangular membership function (MF). The input-output relationships are defined by these rules in form of “If S12 AND S22 then S17”. This process is fulfilled with the help of membership functions (MFs). Decision making unit uses these fuzzy If-Then rules to assign a map from fuzzy inputs to fuzzy outputs based on fuzzy composition rules. Finally, the defuzzification process, Centroid defuzzification in the present study, is used to transfer fuzzy sets into crisp value.

Fig. 3 about here

## *2.2. Multiple linear regression (MLR)*

Regression analysis is used to predict the value of one or more responses from a set of predictors, and also to estimate the linear association between the predictors and responses. Linear regression is a statistical method fitting a linear function of independent variables onto dependent variables by minimizing the least square difference between the predicted and observed values of the data (Draper and Smith 1966). MLR in matrix form can be shown as

(1)

where is regression coefficient matrix, is fitting error matrix and is response matrix. is obtained by solving Equation (1) as follow:

(2)

where is transpose of . In obtaining inverse of, high relativity between independent variables should be avoided, otherwise matrix cannot inverse causing more error. Solution is the avoiding multicollinearity between independent variables. The variance inflated factor (VIF) criterion is usually applied to check multicollinearity. The ideal value for VIF is 1. The higher VIF values mean that the more multicollinearity between independent variables exist (Noori et al., 2010).

## *2.3. Models performance evaluation and validation*

~~The prediction ability of FIS is evaluated~~ The performance of all developed FIS models and MLR was evaluated by using ~~the determination coefficient (R~~~~2~~~~),~~ the mean absolute error (MAE), the Nach-Sutcliffe model efficiency coefficient (NSMEC), and the normalized root mean square error (NRMSE). ~~and the correlation coefficient (CORR). The calculation of R~~~~2~~ ~~is given in Eq. (4):~~

~~(4)~~

~~where represents the observed flow values, represents the predicted flow values, is the mean of the observed flow values and is the mean of the predicted flow values.~~The output of these analysis helps to select best model among developed models. MAE is a common measure of forecast error in time series to determine how developed model outputs fit the observed data. The formula of MAE is shown in Eq. (3):

(3)

where represents the observed flow values, represents the predicted flow values, is the number of flow values.

The ~~NSSS~~ NSMEC is commonly used to assess the predictive power of hydrological discharge models. It is defined as:

~~NSSS~~ (4)

where mean of observed flow values. The ~~NSSS~~ NSMEC can range from to 1. An ~~NSSS~~ NSMEC equal to 1 means there is a perfect match between the model and the observations.

The NRMSE statistic indicates a model’s ability to predict a value away from the mean. The NRMSE is calculated by Eq. (5):

(5)

~~The correlation coefficient (CORR) is a commonly used statistic for providing information about the strength of the relationship between the observed and the predicted data. If this criterion equals zero, then the model represents a perfect fit, which is categorically impossible. The CORR is calculated as in Eq. (7):~~

~~(7)~~

Splitting available data (or record) into two segments; one of which is used for calibration (or training) and the other for validation, is the usual/straightforward method applied for model validation. However, this is possible when the available data is sufficient and can meaningfully split. This splitting procedure can be done as one half for calibration and other for validation if data is long enough, or can be done as 70% of data for calibration and 30% of data for validation (Klemeš, 1986). In the present study, since we are modelling prediction of flood hydrographs, 2010 flow data covering flood period was used for calibration (corresponding about 73% of all data) and 2012 flow data covering flood period (about 27% of all data) was used for validation.

## ~~2.3 Data and model application~~

~~The Maritza River, which is 490 km long, originates at 2400 m a.s.l in the Rila Mountains (Bulgaria) and flows southeast for 320 km (Fig. 2). The catchment of the Maritza River has an area of 52600 km~~~~2~~~~, 28% of which is located in Turkey. After flowing along a short portion of the Greek‒Bulgarian border, the river arrives in Turkey, where it flows for 13 km, after which it forms the border between Turkey and Greece until it disembogues into the Aegean Sea (Yıldız et al., 2014). The Maritza basin is under the influence of both the continental and the Mediterranean climates. The high flow period for the regions under the continental climatic influence can be observed in the northern part of Maritza basin and comes in late spring. On the other hand, the Mediterranean climatic influence is more visible to the south, affecting the lower parts of the Maritza and causing high flow conditions during winter (Tuncok, 2015). Flooding of the Maritza River typically occurs in the autumn, winter, and spring seasons and is caused mainly by heavy rainfalls and snowmelts (Tuncok, 2015).~~

~~In the present study, flow data from the Plovdiv and Svilengrad stations (Bulgaria), and the Kirişhane station (Turkey), all located on the Maritza River, were gauged every two hours covering the period from 9 February 2010 00:00:00 to 21 February 2010 22:00:00. These data were used to predict current streamflow via FIS. Figure 3 shows the two hourly streamflow data including the 159 rows used in this study. An example of one day’s worth of data is given in Table 1.~~

~~In the study, four different models were developed for the prediction of the current flow of the Kirişhane station (Q\_K~~~~i~~~~) using the transboundary data of the Plovdiv and Svilengrad stations. To this aim, the FIS editor graphical user interface (GUI) toolbox in the MATLAB/Simulink program was used. In the first model, Q\_K~~~~i~~ ~~was estimated using the current flows of the Plovdiv (Q\_P~~~~i~~~~) and the Svilengrad (Q\_S~~~~i~~~~) stations. In the second model, Q\_K~~~~i~~ ~~was estimated based on a two hour ahead predicted flow of the Svilengrad station (Q\_S~~~~i-2~~~~) and a four hour ahead flow prediction of the Plovdiv station (Q\_P~~~~i-4~~~~). In the third model, Q\_K~~~~i~~ ~~was estimated based on a four hour ahead predicted flow of the Svilengrad station (Q\_S~~~~i-4~~~~) and an eight hour ahead flow prediction of the Plovdiv station (Q\_P~~~~i-8~~~~). In the last model, Q\_K~~~~i~~ ~~was estimated based on a six hour ahead predicted flow of the Svilengrad station (Q\_S~~~~i-6~~~~) and a twelve hour ahead predicted flow of the Plovdiv station (Q\_P~~~~i-12~~~~). All developed models are shown in Table 2.~~

~~All four models were based on the Mamdani model, in which both input and output variables are fuzzified. The triangular membership function was selected for the two inputs (flows of Plovdiv and Svilengrad stations) and one output (flow of Kirişhane station) of the models (Fig. 3). The ranges of inputs and output variables were divided into fuzzy regions which included S~~~~N~~ ~~(Small N),…, S1 (Small 1), CE (Center), B~~~~1~~ ~~(Big 1),…, B~~~~N~~ ~~(Big N). The number of membership functions were increased in all models until the best result was obtained. The number of membership functions used in all models was the same for the two inputs and one output. In total, 26 membership functions were defined. After determination of the degrees of the data in different regions in which numbers can be different, the fuzzy rules of the models were generated by using AND logical conjunction (Fig. 4). The centroid defuzzification procedure was employed to obtain the predicted flow value of the output based on the fuzzy rule base. The performances of the developed models were then compared. Figure 5 depicts examples of fuzzy rules developed in the models.~~

## *2.4. Structure of forecasting models and application*

In the study, four different models were developed for the prediction of the flood hydrograph of the Kirişhane station (Q\_Ki) using the transboundary data of the Plovdiv and Svilengrad stations. In the first model, Q\_Ki was estimated using the current flows of the Plovdiv (Q\_Pi) and the Svilengrad (Q\_Si) stations. In the second model, Q\_Ki was estimated based on a two hour ahead predicted flow of the Svilengrad station (Q\_Si-2) and a four hour ahead flow prediction of the Plovdiv station (Q\_Pi-4). In the third model, Q\_Ki was estimated based on a four hour ahead predicted flow of the Svilengrad station (Q\_Si-4) and an eight hour ahead flow prediction of the Plovdiv station (Q\_Pi-8). In the last model, Q\_Ki was estimated based on a six hour ahead predicted flow of the Svilengrad station (Q\_Si-6) and a twelve hour ahead predicted flow of the Plovdiv station (Q\_Pi-12). All developed models are shown in Table 1.

Table 1 about here

All four models were investigated by MLR and FIS. Here, MLR was selected as simpler data driven forecasting method to show how FIS improves the other simpler forecasting models (such as regression models) and to check whether other simpler data driven models could reach similar results or not. MLR was applied by using IBM SPSS Statistics 24. MLR was investigated for 2010 data as calibration, and for 2012 as validation. For all MLR investigations, multicollinearity of independent variables (i.e. Plovdiv and Svilengrad flow data) was calculated based on VIF criteria which was obtained as close to 1 (as 1,040), means that independent variables are suitable for MLR analysis.

FIS based forecasting was carried out using Mamdani model, in which both input and output variables are fuzzified (Özger, 2009). To this aim, the FIS editor graphical user interface (GUI) toolbox in the MATLAB/Simulink program was used. The triangular MF was selected for the two inputs (flows of Plovdiv and Svilengrad stations) and one output (flow of Kirişhane station) of the models (Fig. 4). According to available dataset, range of memberships was defined between 40 m3s-1 and 200 m3s-1 for Plovdiv, between 100 m3s-1 and 1500 m3s-1 for Svilengrad, and between 400 m3s-1 and 2000 m3s-1 for Kirişhane gauging station. Depending on the ranges of inputs and output variables were divided into different fuzzy regions: 13, 25, and 49 MFs (i.e. S24, S23,..,CE, …, B23, B24) (Fig. 4) to test sensitivity of prediction results to number of MFs and accordingly number of rules. Since ranges of classes for each gauging station data is different due to range of data, class number was increased (from 13 MFs to 49 MFs) until obtaining best results. The equal ranges of class for each membership were defined depending on the number of class (for example; the range of class is 3.2 for Plovdiv due to range of data is 160, and number of class is 50 as a result of narrow classification of flow data depending on ranges defıned). The fuzzy rules of the models were generated by using AND logical conjunction. This process was separately made for each model by filtering classified flow data in MS Excel until remains unique rules in the form of “If S12 AND S22 then S17”, thus different number of rules was obtained. The centroid defuzzification procedure was employed to obtain the predicted flow value of the output based on the fuzzy rule base. Model validation was made and then the performances of the developed models were compared.

Fig. 4 about here

# 3. Results and discussion

~~The FIS was used to predict the current flow of the Kirişhane station from the transboundary data of the Plovdiv and Svilengrad stations on the Maritza River. To this aim, four different models were developed. The results of the developed models graphically shown in Fig. 6 were compared in terms of prediction performance. The NSSS, R2, NRMSE, and CORR were used to evaluate the prediction performance of the models. For comparison, charts resulting from observed and predicted values for all models can be seen in Fig. 7.~~

~~A summary of the results of the performance criteria of the models is given in Table 3. According to the performance criteria of the models, all the developed models produced very satisfactory results. Among the developed models, M2 gave the best results according to both NSSS and R2 values, whereas M4 had the lowest NSSS and R2 values. According to the NRMSE criteria, M2 gave the best result. According to the CORR statistic, although all the developed models had similar values, a stronger relationship was observed between the predicted and observed values in M4. In all developed models, the same number of triangular membership functions (equal to 26) was used. Except for M3, the number of fuzzy rules written in all models was the same as seen in Table 3.~~

In the present study, FIS models with different number of MFs (13 MFs, 25 MFs, and 49 MFs) and MLR were developed to predict the flood hydrograph of the Kirişhane station from the transboundary flow data (belonging to 2010 and 2012 floods) of the Plovdiv and Svilengrad stations on the Maritza River and test the obtained results for comparison with respect to prediction accuracies. Streamflow is gauged in normal at eight hour-intervals along one year, however, flow data is also gauged at two hour-intervals only for flood periods. That’s why flow data used in the present study is limited with several days. While 2010 flow data was used for construct models, 2012 flow data was used to validate models. Flow data used as test data is less than training data because test data could be gauged only during recession period of flood. Maritza River has two main tributaries (Arda and Tundja) located between Svilengrad and Kirişhane gauging stations. Detailed information on Maritza, Arda, and Tundja Rivers and their tributaries can be found in Tuncok et al., (2014). And also, distance between Svilengrad and Kirişhane (about 45 km) is quite short relative to distance between Plovdiv and Svilengrad (about 180 km). That’s why, high differences of flows between gauging stations are available due to contributions from Arda and Tundja Rivers.

Three different criteria were used to test performance of each model (MAE, NSMEC, and NRMSE). A summary of the results of the performance criteria of the models is given in Table 2. According to the performance criteria of the models, FIS model with 49 number of MFs provided highest accuracy. When FIS models with 25 MFs and 49 MFs are compared with respect to performance criteria for 2010 data (training data), NSMEC values are close to each other, but MAE values of FIS models with 49 MFs were obtained less than FIS model with 25 MFs. Even though NSMEC values were obtained close to each other for FIS models with 25 MFs and 49 MFs, NSMEC values of FIS model with 25 MFs were obtained less than 0.90 for 2012 data (validation data). With respect to MLR, all models failed to predict 2012 data, even NSMEC values were obtained higher than 0.85 for training data. All FIS models with 13 MFs provided better prediction of 2012 data than MLR. This is most probably due to limited data availability used in model construction. Even so, all FIS models applied in the study can predict flood hydrograph better than MLR. That’s why, it is possible to say that FIS as a soft computing technique in prediction of flood hydrograph or streamflow is more powerful technique than simpler statistical methods (such as MLR). But this doesn’t mean that the existence of statistical methods can be denied (Kar et al., 2010)

Table 2 about here

In the present study, fuzzy rules were generated by filtering classified flow data to generate MFs until unique fuzzy rules in the form of “If S12 AND S22 then S17” remain. The procedure of generating rules applied in the present study is quite easy and provides all possible fuzzy rules for available flow data of three gauging stations in construction of the models. Due to high number of MFs (such as 25 and 49) depending on class range of flow data, and variation in the data distribution in each class, different (and high) number of fuzzy rules (varying from 44 to 167) were obtained for each FIS models. In the present study, albeit the high number of fuzzy rules can be seen as an artifact, the best prediction accuracies could only be obtained by defining high number of MFs (i.e. 49 MFs) and accordingly high number of fuzzy rules (more than 150 fuzzy rules). In the literature, examples of high number of fuzzy rules are also available: for instance, Turan (2007) generated fuzzy models with 19 MFs resulting in 75 fuzzy rules. Obtaining the best results from FIS generated by high number of fuzzy rules is probably due to the nonlinearity of flood hydrograph, differences in the flows between each gauging station, and the range of minimum and maximum flow of each gauging. When compared number of flow data, the number of rules seems to be equal to (even more) flow data, because of availability of flow data for only two years (2010 and 2012) which limits the construction of a general (global) model for Maritza River to predict flood hydrograph. In order to overcome this limitations, re-arrangements in the construction of all models should make by adding additional flow data will be gauged for future flood periods. The results of the FIS with 49 MFs and MLR models developed using data belongs to 2010 and 2012 are given graphically in Fig. 5. In addition, charts resulting from observed and predicted values for all models developed with FIS with 49 MFs using data belongs to 2010 and 2012 are given in Fig. 6.

Fig. 5 about here

Fig. 6 about here

# 4. Conclusions

~~The main objective of the present study was to employ FIS for the prediction of the current flow of the Kirişhane station from the transboundary data of the Plovdiv and Svilengrad stations on the Maritza River. For this task, four different models were developed. In the first model, an estimation was made using current flows of the Plovdiv and Svilengrad stations. In the second model, an estimation was made based on a two hour ahead flow prediction of the Svilengrad station and a four hour ahead flow prediction of the Plovdiv station. In the third model, a calculation was based on a four hour ahead flow prediction of the Svilengrad station and an eight hour ahead flow prediction of the Plovdiv station. In the last model, an estimation was based on a six hour ahead flow prediction of the Svilengrad station and a twelve hour ahead flow prediction of the Plovdiv station.~~

~~The models with the best fit were selected based on the values of a series of performance measures that included the R2, the NSSS, the NRMSE, and the CORR. The results for each of the models are shown in Table 3. Based on these values, it can be observed that all the models developed were capable of yielding satisfactory predictions. According to the performance criteria of the developed models, M2 had a better prediction performance than the others. Model M2 predicted the current discharge of the Kirishane station two hours ahead of the Svilengrad station and four hours ahead of the Plovdiv station.~~

~~The Maritza River, which is the biggest river on the Balkan Peninsula, affects Turkey, Greece, and Bulgaria. In particular, the lower regions of the Maritza River have suffered from floods. In this regard, although early warning systems offer the population time to evacuate before floods, improving early warning systems involves multiple components, each with a cost. Furthermore, long-term observation of the hydro-meteorological conditions of the floods is needed. Hence, developed models are crucial in the prediction of current flows. Doing nothing is not an option; thus, this study has shown that developed fuzzy rule-based models can satisfactorily predict the flow regime with high accuracy and therefore can be used to develop a reliable flow forecasting system. Moreover, in practice, such studies may be used to apply the values of upstream stations for the estimation of the missing values of downstream stations.~~

The Maritza River, which is the biggest river on the Balkan Peninsula, affects Turkey, Greece, and Bulgaria. The Maritza River has two main tributaries (Arda and Tundja Rivers) located between Svilengrad and Kirişhane gauging stations which cause an increase in flow. These three rivers are international shared water bodies in the Balkan Peninsula. The lower regions of the Maritza River (especially Edirne city and surrounding regions) have suffered from floods. Streamflow or flood forecasting has become very demanding task in mitigation of effects of floods on human and dam safety as well as on ecosystem sustainability. Soft computing techniques have become common techniques in prediction streamflow or flood. That’s why, the main objective of the present study was to employ FIS for the prediction of the flood hydrograph of the Kirişhane station from the transboundary data of the Plovdiv and Svilengrad stations on the Maritza River. For this aim FIS models with different MFS (13 MFs, 25 MFs, and 49 MFs) and also MLR were selected to predict flood hydrograph. Prediction performances of all models was evaluated by using three criteria: MAE, NSMEC, and NRMSE. Because flow data used in the study is available at two hour-intervals for only flood period (in this study, only flow data of 2010 and 2012 years is available), prediction was made by using limited data. With respect to model construction this can be a limitation since it limits the representation power of models for flood behaviors rising from Maritza River. That’s why, developed models should re-arrange by using additional flow data which will be obtained from future flood events. Because fuzzy models can be easily modified dynamically depending on whether addition data is available or not. Even though flow data belonging to only two years available, FIS models provided predictions with high values of NSMEC. All FIS models provided higher prediction accuracies than MLR, and MLR method failed to predict test data (2012 flow data). Of course, it must keep in mind that availability of more flow data in the model construction phase will provide more reliable results. This study demonstrated that FIS models can be successfully applied for prediction of flood hydrograph. Another important point in the study is the usage of transboundary flow data from different three gauging stations (Plovdiv, Svilengrad, and Kirişhane), two of them is located in Bulgaria.

# References

Alvisi, S., Mascellani, G., Franchini, M., and Bardossy, A.: Water level forecasting through fuzzy logic and artificial neural network approaches, Hydrology and Earth System Sciences, 10, 1–17, 2006.

Amisigo, B.A., van de Giesen, N., Rogers, C., Andah, W.E.I., and Friesen, J.: Monthly streamflow prediction in the Volta Basin of West Africa: A SISO NARMAX polynomial modelling, Physics and Chemistry of the Earth, 33, 141–150, 2008.

Altunkaynak, A., Özger, M., and Çakmakçi, M.: Water consumption prediction of Istanbul city by using fuzzy logic approach, Water Resources Management, 19, 641‒654, 2005.

Aydın, A., and Eker, R.: Prediction of daily streamflow using Jordan-Elman networks, Fresenius Environmental Bulletin 21:1515‒1521, 2012.

Batur, E., and Maktav, D.: Floodplain Assessment with the Integration of Remote Sensing and GIS: Meric River Case Study (original in Turkish), Havacilik ve Uzay Teknolojileri Dergisi, 5(3), 47‒54, 2012.

Besaw, L.E., Rizzo, D.M., Bierman, P.R., and Hackett, W.R.: Advances in ungauged streamflow prediction using artificial neural networks, Journal of Hydrology, 386, 27–37, 2010.

Campolo, M., Andreussi, P., and Soldati, A.: River flood forecasting with a neural network model. Water Resources Research, 35(4), 1191-1197, 1999.

Chaloulakou, A., Assimakopoulos, D., and Lekkas, T.: Forecasting daily maximum ozone concentrations in the Athens basin, Environmental Monitoring and Assessment, 56, 97-112, 1999.

Chang, F.J., and Chen, Y.C.: A counter propagation fuzzy-neural network modelling approach to real time streamflow prediction, Journal of Hydrology, 245, 153‒164, 2001.

Chen, S.H., Lin, Y.H., Chang, L.C. and Chang, F.J.: The strategy of building a flood forecast model by neuro-fuzzy network, Hydrol. Processes, 20: 1525–1540, 2006.

Cigizoglu, H.K.: Estimation, forecasting and extrapolation of river flows by artificial neural networks, Hydrological Sciences, 48 (3), 349–361, 2003.

Draper, N.R. and Smith, H.: Applied Regression Analysis. John Wiley and Sons, 709 pp,1966.

Elsayed, T.: Fuzzy inference system for the risk assessment of liquefied natural gas carriers during loading/offloading at terminals, Applied Ocean Research, 31, 179-185, 2009.

Firat, M., Comparison of artificial intelligence techniques for river flow forecasting, Hydrology and Earth System Sciences, 12, 123–139, 2008.

Firat, M., and Gungor, M.: Hydrological time-series modelling using an adaptive neuro-fuzzy inference system. Hydrological Processes 22, 2122–2132, 2008.

Garcia-Bartual, R.: Short term river forecasting with Neural Networks, Integrated Assessment and Decision Support. Proc. 1st biennal meeting Int. Environmental Modelling and Software Society, 2, 160-165, 2002.

Govindaraju, R.S.: Artificial neural networks in hydrology II: hydrogeologic applications, Journal of Hydrologic Engineering, 5 (2), 124–137, 2000.

Hong, T.P., and Lee, C.Y.: Induction of fuzzy rules and membership functions from training examples, Fuzzy Sets and Systems, 84, 33–47, 1996.

Jamshidi, A., Yazdani-Chamzini, A., Yakhchali, S.H., and Khaleghi, S.: Developing a new fuzzy inference system for pipeline risk assessment, Journal of Loss Prevention in the Process Industries, 26, 197-208, 2013.

Jang, J. S. R.: Anfis: Adaptive-network-based fuzzy inference system, IEEE Transactions on Systems, Man, and Cybernetics 23 (3), 665–685, 1993.

Kar A.K., Lohani, A.K., Goel, N.K., and Roy G.P.: Development of Flood Forecasting System Using Statistical and ANN Techniques in the Downstream Catchment of Mahanadi Basin, India. J. Water Resource and Protection, 2, 880-887, 2010.

Klemeš, V.: Operational testing of hydrologic simulation models, Hydrol. Sci. J., 31, 13-24, 1986.

Küçük, M., and Ağıralioğlu, N.: Wavelet Regression Technique for Streamflow Prediction, Journal of Applied Statistics, 33(9), 943‒960, 2006.

Lekkas, D.F., Onof, C., Lee, M.J., and Baltas, E.A.: Application of Artificial Neural Networks for Flood Forecasting, Global Nest: the Int. J., 6(3), 205‒211, 2005.

McKerchar, A.I., and Delleur, J.W.: Application of seasonal parametric linear stochastic models to monthly flow data, Water Resour. Res., 10 (2), 246–255, 1974.

Mukerji, A., Chatterjee, C., and Raghuwanshi, N.S.: Flood forecasting using ANN, Neuro-Fuzzy, and Neuro-GA Models. Journal of Hydrologic Engineering, 14(6), 647-652, 2009.

Nayak, P.C., Sudheer, K.P., and Ramasastri, K.S.: Fuzzy computing based rainfall–runoff model for real time flood forecasting, Hydrol. Process, 19, 955–968, 2005.

Noori, R., Khakpour, A., Omidvar, B., and Farokhnia, A.: Comparison of ANN and principal component analysis-multivariate linear regression models for predicting the river flow based on developed discrepancy ratio statistic, Expert Systems with Applications, 37(8), 2826-5862, 2010.

Özger, M.: Comparison of fuzzy inference systems for streamflow prediction, Hydrological Sciences Journal, 54(2), 261‒273, 2009.

Rezaeianzadeh, M., Tabari, H., Yazdi, A.A., Isik, S., and Kalin, L.: Flood flow forecasting using ANN, ANFIS and regression models. Neural Comput & Applic, 25, 25-37, 2014.

Sezen, N., Gündüz, N., and Malkaralı, S.: Meriç River Floods and Turkish-Bulgarian Cooperations, International Congress on River Basin Management, 646‒654, 2007.

Şen, Z., and Altunkaynak, A.: Fuzzy system modeling of drinking water consumption prediction, Expert Systems with Applications, 36, 11745‒11752, 2009.

Takagi, T., and Sugeno M.: Fuzzy identification of systems and its applications to modeling and control. IEEE Transactions on Systems, Man, and Cybernetics, 15 (1), 116-132, 1985.

Tokar, AS, and Markus M.: Precipitation-runoff modeling using artificial neural networks and conceptual models. Journal of Hydrologic Engineering, ASCE, 5(2): 156–16, 2000.

Tuncok, I.K.: Transboundary river basin flood forecasting and early warning system experience in Maritza River basin between Bulgaria and Turkey, Nat. Hazards, 75, 191–214, 2015.

Turan, M.E.: The use of artificial intelligence techniques in prediction of streamflow (original in Turkish), Master Thesis, Celal Bayar University, pg 93, 2007.

Turan, E.M., and Yurdusev, M.A.: River flow estimation from upstream flow records by artificial intelligence methods, Journal of Hydrology, 309, 71‒77, 2009.

Wang, Y.C., Chen, S.T., Yu, P.S., and Yang, T.C.: Storm-even rainfall–runoff modelling approach for ungauged sites in Taiwan. Hydrological Processes, 22, 4322–4330, 2008..

Yen, J., and Langari, R.: Fuzzy Logic: Intelligence, Control and Information, Prentice Hall, 1999.

Yıldız, D., Özbay, Ö., Çakmak, C., and Soylu, N.: International water management in the Maritza Catchment (original in Turkish), Report 2, Hydropolitics Academy, Ankara, 2014.

Yurekli, K., Kurunc, A., and Ozturk, F.: Application of linear stochastic models to monthly flow data of Kelkit Stream, Ecological Modelling, 183, 67–75, 2005.

Table 1. Developed models, inputs and output

|  |  |  |
| --- | --- | --- |
| Model Name | Inputs | Output |
| M1 | Q\_Pi, Q\_Si | Q\_Ki |
| M2 | Q\_Pi-4, Q\_Si-2 | Q\_Ki |
| M3 | Q\_Pi-8, Q\_Si-4 | Q\_Ki |
| M4 | Q\_Pi-12, Q\_Si-6 | Q\_Ki |

Table 2. Results of performance criteria of developed models

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Method | Data | Models | Number  of  Membership | Number  of  Rules | MAE | NSMEC | NRMSE |
| FIS | 2010 | M1 | 49 | 165 | 30.6090 | 0.9803 | 0.0473 |
| M2 | 167 | 33.1532 | 0.9719 | 0.0560 |
| M3 | 162 | 30.9322 | 0.9691 | 0.0584 |
| M4 | 156 | 36.3203 | 0.9545 | 0.0671 |
| M1 | 25 | 100 | 55.6436 | 0.9572 | 0.0697 |
| M2 | 90 | 55.9396 | 0.9487 | 0.0757 |
| M3 | 90 | 49.0908 | 0.9621 | 0.0646 |
| M4 | 93 | 46.8804 | 0.9540 | 0.0691 |
| M1 | 13 | 63 | 80.1455 | 0.9173 | 0.0968 |
| M2 | 44 | 75.3396 | 0.9238 | 0.0923 |
| M3 | 44 | 71.2151 | 0.9288 | 0.0886 |
| M4 | 46 | 61.7500 | 0.9356 | 0.0833 |
| 2012 | M1 | 49 | 165 | 31.0532 | 0.9410 | 0.0535 |
| M2 | 167 | 24.0356 | 0.9649 | 0.0391 |
| M3 | 162 | 15.8698 | 0.9826 | 0.0265 |
| M4 | 156 | 23.2205 | 0.9297 | 0.0463 |
| M1 | 25 | 90 | 59.5447 | 0.8395 | 0.0883 |
| M2 | 90 | 55.9600 | 0.8207 | 0.0864 |
| M3 | 90 | 46.4953 | 0.8504 | 0.0776 |
| M4 | 93 | 49.2769 | 0.8070 | 0.0766 |
| M1 | 13 | 44 | 78.8702 | 0.7746 | 0.1046 |
| M2 | 44 | 68.9400 | 0.7878 | 0.0940 |
| M3 | 44 | 65.3140 | 0.7367 | 0.1029 |
| M4 | 46 | 75.4179 | 0.5483 | 0.1172 |
| MLR | 2010 | M1 | - | - | 100.0620 | 0.8512 | 0.1298 |
| M2 | - | 92.2652 | 0.8747 | 0.1183 |
| M3 | - | 87.7735 | 0.8917 | 0.1092 |
| M4 | - | 81.2091 | 0.8981 | 0.0977 |
| 2012 | M1 | - | - | 532.3520 | -7.4908 | 0.6419 |
| M2 | - | 528.9981 | -8.5761 | 0.6460 |
| M3 | - | 457.8676 | -9.1119 | 0.6378 |
| M4 | - | 436.0640 | -9.3782 | 0.5618 |




Figure 1. Location map of Maritza River

|  |
| --- |
| 2010 |
| 2012 |
| Figure 2. Flow data belongs to 2010 and 2012 years for all stations in the study |




Figure 3. Fuzzy inference system (FIS)




Figure 4. Example depiction of triangular MFs of flow data (Plovdiv station)

|  |  |
| --- | --- |
| 2010 | 2012 |
| 2010 | 2012 |
| 2010 | 2012 |
| 2010 | 2012 |
| Figure 5. Graphical depiction of the results of Models 1 – 4 for 2010 and 2012 years using FIS with 49 MFs and MLR | |

|  |  |
| --- | --- |
| 2010 | 2012 |
| 2010 | 2012 |
| 2010 | 2012 |
| 2010 | 2012 |
| Figure 6. Resulting scatterplots of observed and predicted values of developed FIS models with 49 MFs for 2010 and 2012 years | |